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      DOOSAN MX 2500 ST Multi Axis Turning
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· Make

: DOOSAN - Korea
· Type

: MX 2500 ST  
· Serial NO
: PX 25 ST 0109 + 0087
· Age

: 2005
· Max. swing Ø
:   850
· Machining swing Ø
:   540
· Spindle bore Ø
:    65
· X 1 travel

:   555
· X 2 travel

:   185

· Y travel

:   160
· Z 1 travel

: 1.095
· Z 2 travel

: 1.140

· A travel

: 1.065

· Left spindle

· Speed 

: 3.500
· Spindle bore
:     76

· C axis indexing
: 360.000

· Power


: 26 kW

· Right spindle

· Speed 

: 3.500

· Spindle bore
:     76

· C axis indexing
: 360.000

· Power


: 26 kW

· Milling spindle


· Speed

: 10.000

· B Axis

: 240

· Indexing

: 0.001 Gr

· Chain ATC 

: 40 positions

· Power


: 18.5 kW

· Tool size
Ø
: 90 x 300 x 8 Kg


· Lower revolver

· Number off station
:      12

· Speed live tools

: 4.000

· Boring bar Ø

:     40

· OD tool size


:     25

· Live tools 


: 5.5 kW
· Feed rate X


: 24.000
· Feed rate Z


: 24.000
· Feed rate Y 


: 16.000
· Feed rate A


: 24.000
· Dimensions

· Length

: 5.500
· Width

: 2.300
· Height

: 2.600
· Weight

: 12.500
· Power


: 93.92 kVa

· CNC Fanuc 18 I TB

· Chip conveyor

· Coolant system

· Tool eye

· Double Kitagawa Chuck B 210 ? 

· Documentation

Please Note: The above information has been obtained to the best of our ability and belief from, and from the manufacturers where possible. It is given in good faith, but its accuracy can not be guaranteed. Accordingly, it will not form a representation or constitute contractual terms. We advise you to check any vital details
Transito 21, 6909 DA Babberich, Netherlands


Tel. + 31 (0)316 – 247123


Fax. + 31 (0)316 - 247956


www.mach4metal.com





Bank No : 66.52.13.883


IBAN    : NL33 INGB 0665 2138 83


BIC      : INGBNL2A


VAT	   : NL 815393635B01





�











�





�





�








