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 Centre hole grinder TECHNICA Z Axis CNC
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Make

: TECHNICA Swiss
· Typ

: ZSM 5100 - 815
· Mach. No
: J 20339
· Age

: 2003 rebuild
· Centre hole  Ø Min
  
:   3        
· Centre hole  Ø Max.
: 60
· Length workpiece
Min.     :    50
· Length workpiece  Max.
 : 1.100
· Workpiece weight
Kg
 :   120 

· Clamp range vice

: Ø 4 - 140
· Grinding wheel spindle     : Ø        32
· Ø 15
- 45.000 Rpm

· Ø 27
- 22.500 Rpm

· Ø 48
- 13.000 Rpm

· Ø 60
- 13.000 Rpm

· Grinding head adjustment  : 160
·  Rapid head adjustment
   :  70

· Automatic dressing stroke : 40

· Adjustment
: 0.01 – 0.03 mm

· Dressing speed Diamond
: 470 mm/Min

· Dimensions
· Length
:   967

· Width
:   856

· Height
: 1.850

· Weight
:   700
· Z Axis over CNC programmable !
Please Note: The above information has been obtained to the best of our ability and belief from, and from the manufacturers where possible. It is given in good faith, but its accuracy can not be guaranteed. Accordingly, it will not form a representation or constitute contractual terms. We advise you to check any vital details!
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