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CNC Rail way lathe Noble & Lund
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· Make

: Noble & Lund
· Typ     
: RL 1400
· Age     
: Retrofitted 2003
· Mach.No. 
: 0920188
· Face plate

: 1.400

· Rail track gauge      : 1.435 mm
· Max. wheel Ø.
  : 1.000 mm
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Min.  wheel Ø.
  :   600 mm
· Max. axle length      : 1.950 mm

· Max. work load
  : 3.600 Kg

· Y Stroke left support : 600
· X Stroke left support :

· Y Stroke right support : 600
· X Stroke right support :
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· Speeds Rpm
:

· Dimensions
· Length
:

· Width
:

· Height
:

· Weight
:

· 2003 new electric cabinet
· 2003 new SIEMENS 840 DI CNC
· 2003 support Central lubrication

Please Note: The above information has been obtained to the best of our ability and belief from, and from the manufacturers where possible. It is given in good faith, but its accuracy can not be guaranteed. Accordingly, it will not form a representation or constitute contractual terms. We advise you to check any vital details![image: image7.jpg]



Transito 21, 6909 DA Babberich, Netherlands


Tel. + 31 (0)316 – 247123


Fax. + 31 (0)316 - 247956


info@mach4metal.com


www.mach4metal.com





Bank No : 66.52.13.883


IBAN    : NL33 INGB 0665 2138 83


BIC      : INGBNL2A


VAT	   : NL 815393635B01
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