MACH4METAL
Metalworking machinery
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Titan Double column vertical lathe
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· Make

: TITAN 
· Typ

: SC 27
· Mach.No
: 126 - 187 
· Age

: OH 2002
· Table size Ø  
:   2.500
· Swing max Ø  
:   2.700
· Turing height 
:   1.900
· Max. workpiece 
: 15.000 kg
· Double support 
· Left ram stroke 
: 
· Right revolver ram   :
· Number off tool revolver :
· Power main SIEMENS 100 kW
· Table rotation 1,24 – 112 Rpm

· Dimensions

· Length

: 4.800
· Width


: 4.800
· Height

: 5.000
· Weight

: 32.000 Kg

· New rittal electric cabinet with new
West European electric / Siemens drive’s

· New SIEMENS Touch panel 

· Rpm / Feed / Rapid / Control X & Z Axis

· Automatic lubrication

· 4 x Clamping jaws

Please Note: The above information has been obtained to the best of our ability and belief from, and from the manufacturers where possible. It is given in good faith, but its accuracy can not be guaranteed. Accordingly, it will not form a representation or constitute contractual terms. We advise you to check any vital details
Account No: 66.52.13.883


IBAN       : NL33 INGB 0665 2138 83


BIC         : INGBNL2A





Transito 21, 


6909 DA BABBERICH, Netherlands


Tel. + 31 (0)316 – 247123


Fax. + 31 (0)316 - 247956


info@mach4metal.com


www.mach4metal.com
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