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Hapremec S.A. CNC Caroussel 
Turning + Grinding machine
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· Make. Hapremec S.A.
· Typ.   VCE 140o
· Mach.No. Sa. 
· Age.   1989
· Table size. Ø. 1.200

· Swing max. Ø. 1.400
· Vertical travel of 
The ram: 550 (on ballscrew)
· Longitudinal travel of 
           the cross-rail: 700 ( on ballscrew) 
· Strokes off spindles: 250 

· Diam. off grinding wheel. Ø 130

· Power spindle motor each. 11 kw

· Number off spindles: 3
· Grinding spindle 1 is fixed 

· Grinding spindle 2 is indexed till 10°

· Turning support    is indexed till 90°

· Dimensions: L x W x H. 

· Machine:           2.700 x 2.400 x 3.950 

· Electr. Cabinet. 2.400 x    400 x 2.000

· Weight. Ca. 11 ton

· Controll Altstohm Cyber 3000

· Incl. manuals / documentation

· Machine ex. Air – France 
Please Note: The above information has been obtained to the best of our ability and belief from, and from the manufacturers where possible. It is given in good faith, but its accuracy can not be guaranteed. Accordingly, it will not form a representation or constitute contractual terms. We advise you to check any vital details!
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